
        
        *****************************************************************************************************************************
        
        The following section should be completed after the BARC has been field validated by the BAER team and this entire metadata file should be returned to GTAC with the Soil Burn Severity data.
        
        Fire name: 4170 TULE RD
        
         
            BAER Assessment Completion Date:
            BAER Team GIS Analyst:
            BAER Team Leader:
            Soil Burn Severity Analyst(s):
            
            Original BARC256 thresholds:
                Unburned / Undetectable: <= 64
                Low: > 64 and <= 131
                Moderate: > 131 and <= 198
                High: > 198
                
            Soil Burn Severity thresholds:
                Unburned / Undetectable:
                Low:
                Moderate:
                High:
                    
            Sequence of steps used to create Soil Burn Severity data:
            
            Additional Comments:
        